Return values are stored in eax register.



































